Basic Workflow
	1	prescanning procedures
	2	calibrate equipment
	3	scan image
	4	archive master
	5	correct image
	6	archive corrected image
	7	optimize image
	8	archive optimized image
	9	add metadata
Prescanning Procedures
	1	check copyright
	2	ensure image has not already been scanned 
Calibrate Equipment
	1	calibrate monitor
	2	scan the colour reference sheet
	3	calibrate scanner based on reference sheet scan
Scanning
	1	clean scanner
	2	determine scanning method 
	2.1	positive print
	2.2	negative
	2.3	transparency
	3	set scanner settings
	3.1	resolution: optical maximum (no interpolation/resampling)
	3.2	colour: RGB / 16bits per channel
	3.3	sharpening: none
	3.4	dust and scratch removal: none
	4	scan image
	4.1	border zone of .25 of an inch
	5	assign colour profile
	sRGB IEC61966-2.1
Archive Master
	1	name: sequential ID number (1, 2, 3...)
	2	file format: uncompressed TIFF
Correct Image
	1	remove any dust or scratches using the clone tool
	2	colour correct image using curves and levels
Archive Retouched Image
	1	name: sequential ID number (1, 2, 3...)
	2	file format: uncompressed TIFF
Create Web Optimized Image
	1	crop file to image area, excluding any page or scanner border
	2	resize to 1500 pixels wide
	3	apply Curves adjustment
	contrast for web (to be supplied)
	4	apply Smart Sharpen filter
	amount: 30%
	radius: 1 pixel
	remove: Gaussian blur
	more accurate: yes
Archive Optimized
	1	name: sequential ID number (1, 2, 3...)
	2	file format: compressed JPG ("save for web")
	2.1	optimized: yes
	2.2	quality: 80%
	2.3	blur: 0
	2.4	include ICC Profile: no 
	2.5	progressive downloading: no
	2.6	matte: none
Folder Structure
	/digitization/
	/digitization/masters/
	/digitization/retouched/
	/digitization/optimized/